UDecide

CUSTOMER REQUIREMENTS SPECIFICATION  
DOCUMENT REFERENCE NUMBER: UD-CRS  
  
DATE: 23-03-2021  
 REVISION NUMBER: 2.0

*AUTHOR:* Emma Elbo & Amalie Koch.

*REVIEWER:* Sigrid Stang & Sofie Bjørn.

SCOPE: This document contains customer requirements for the UDecide information system.

REFERENCES:

REVISION HISTORY:

|  |  |  |  |
| --- | --- | --- | --- |
| **Revision** | **Revised by** | **Revision date** | **Description of changes** |
| 1.0 | Sigrid Stang, Sofie Bjørn, Emma Elbo & Amalie Koch | 16-03-2021 | First version |
| 2.0 | Emma Elbo & Amalie Koch | 23-03-2021 | The customer requirement specification has been updated based on the information collected from a meeting with InnoCon Medical and based on an interview with a Gynecologist. |
|  |  |  |  |

APPROVAL:

|  |  |  |  |
| --- | --- | --- | --- |
|  | *Name and job function* | *Signature* | *Date* |
| *Author:* |  | | |
| *Reviewer:* |  | | |
| *Independent reviewer:* |  | | |

**Custumer requirement specification**

|  |  |
| --- | --- |
| **UD-CRS-ID** | **CUSTOMER REQUIREMENT SPECIFICATION** |
| UD-CRS-01 | The UDecide system shall assist the specialist in clinical practice in choosing the most beneficial stimulation paradigm |
| UD-CRS-02 | The UDecide system shall be compatible with the product UCon, by InnoCon Medical |
| UD-CRS-03 | The UDecide system shall have a simple graphical user interface to the specialist in clinical practice |
| UD-CRS-04 | The UDecide system shall be simple to integrate in the current workflow and in the clinical environment |
| UD-CRS-05 | The UDecide system shall be based on an algorithm, that takes in inputs which are already registered in clinical practice. |
| UD-CRS-06 | The output of the UDecide system shall support the dialog between the specialist and the patient when deciding which stimulation paradigm should be used in the treatment |
| UD-CRS-07 | The output of the UDecide system shall show an “effectiveness score” to support the specialist |
| UD-CRS-08 | The output of the UDecide system concerning stimulation paradigm shall be compatible with the stimulation possibilities that the UCon stimulator provide |
| UD-CRS-09 | The UDecide system shall be able to update the algorithm periodically based on data from UCon |
| UD-CRS-10 | The UDecide system shall be able to take patient preferences as an input to the algorithm |
| UD-CRS-11 | The output of the UDecide system shall weight the output, so that a minimal stimulation relative to high effect is weighted as the most beneficial stimulation paradigm |